Linux - Panasonic LF1000 Optical Disk mini HOWTO

Skip Rye

root@brspc_0061.msd.ray.com

Mamoto Yoshinori - 彺栿丒廋惓

ymamoto@ent.med.osaka-u.ac.jp

v1.1, March 29, 1996

LF1000 (PD) 傪 Linux 偱巊偆丅

 

   
    Note: 偙偺僼傽僀儖偼丄IBM PC 屳姺婡忋偺僔僗僥儉偵偺傒摉偰偼傑傝傑偡
    丅尨暥偱偍偐偟側愝掕傪偟偰偄傞偲巚傢傟傞晹暘偼丄揔媂曄峏偟偰偁傝傑
    偡丅
   
 

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

Table of Contents
1. Legal notice
   
    1.1. 柶愑帠崁
    1.2. 挊嶌尃
   
2. 偼偠傔偵
   
    2.1. 岝憡曄壔媄弍
    2.2. 棙揰
    2.3. 棟夝偟偰梸偟偄帠
   
3. 僀儞僗僩乕儖
   
    3.1. 僀儞僗僩乕儖偺庤弴
    3.2. 僸儞僩
   
4. 捛壛丒曗懌

1. Legal notice

1.1. 柶愑帠崁

偙偺 HOWTO 暥彂偺挊幰偍傛傃攝晍幰偼丄偙偺暥彂偺撪梕偵傛偭偰堷偒婲偙偝傟
傞偄偐側傞椶偺暔棟揑丄嬥慘揑丄惛恄揑懝奞偵懳偟偰傕丄堦愗偺愑擟傪晧傢側
偄偙偲傪偙偙偵愰尵偟傑偡丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

1.2. 挊嶌尃

偙偺暥彂偼丄Skip Rye 偵挊嶌尃(1996擭)偑偁傝傑偡丅Linux HOWTO 暥彂偼丄挊
嶌尃昞婰傪巆偟偰偁傝偝偊偡傟偽丄偦偺堦晹傕偟偔偼慡懱傪丄偄偐側傞儊僨傿
傾偱攝晍偟偰傕峔偄傑偣傫丅彜梡攝晍傕峔偄傑偣傫偟丄墳墖偟偰偄傑偡丅偟偐
偟丄偙偺暥彂偺攝晍偵娭偟偰拲堄帠崁偑偁傝傑偡丅Linux HOWTO 暥彂偺撪梕傪
娷傓丄偁傜備傞東栿暔丄攈惗暥彂丄傑偲傔傕丄偙偺挊嶌尃婯栺偵廬偆昁梫偑偁
傝傑偡丅偄偄偐偊傟偽丄偙偺婯栺埲奜偺忦審傪晅偗偨宍偱偺攝晍傪偟偰偼偄偗
側偄偲偄偆偙偲偱偡丅偙偺婯栺偺椺奜偼丄摿掕偺応崌偺傒嫋偝傟傑偡丅梫偡傞
偵偙偺忣曬傪偱偒傞偩偗懡偔偺僠儍儞僱儖傪捠偟偰峀傔偨偄偺偱偡丅巹偨偪偼
丄 HOWTO 暥彂偺挊嶌尃傪曐帩偟傛偆偲巚偭偰偼偄傞傕偺偺丄嵞攝晍偡傞偨傔偺
偄偐側傞寁夋傕峫偊偰偼偄傑偣傫丅傕偟丄壗偐幙栤偑偁傟偽丄Linux HOWTO 暥
彂娗棟幰偺 Greg Hankins 偵丄E-mail:gregh@sunsite.unc.edu 埗偱楢棈傪偲偭
偰偔偩偝偄丅揹榖斣崋傪嫵偊偰傕傜偄丄偝傜偵徻偟偄忣曬傪摼傜傟傞偐傕偟傟
傑偣傫丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

2. 偼偠傔偵

2.1. 岝憡曄壔媄弍

乽岝憡曄壔媄弍乿偼丄憡曄壔彂偒崬傒偺偨傔偺摿庩側儊僨傿傾忋偵丄乽寢徎忬
懺乿偲乽傾儌儖僼傽僗忬懺乿偲傪嶌傝偩偟丄偦偺憡堘傪價僢僩僨乕僞偲偟偰埖
偆媄弍偱偡丅偙偺偨傔偵丄憡曄壔僪儔僀僽偼丄僄僱儖僊乕儗儀儖偺堎側傞儗乕
僓乕傪巊梡偟偰丄偙偺忬懺傪曄壔偝偣傞傛偆偵側偭偰偄傑偡丅寢徎壔偟偰偄傞
椞堟偼丄傾儌儖僼傽僗壔偟偰偄傞椞堟偲丄撉傒崬傒梡偺儗乕僓乕偺斀幩棪偑堎
側傞偙偲傪棙梡偟偰丄僨傿僗僋偐傜僨乕僞偑撉傒偙傔傞傢偗偱偡丅

岝憡曄壔僨傿僗僋偑摿暿側偺偼丄帴婥僨傿僗僋傗岝僨傿僗僋偲摨偠偔丄摨怱墌
忬偺僩儔僢僋丒僙僋僞宍幃偱僼僅乕儅僢僩偝傟偰偄傞傕偺偺丄奺僩儔僢僋偼丄
旕忢偵崅枾搙偵暲傫偱偄傞偺偱丄堦枃偺僨傿僗僋偵嬌傔偰戝検偺僨乕僞偑婰榐
偱偒傞傛偆偵側偭偰偄傞揰偱偡丅乮栿拲丗偙傟偠傖丄摿暿偱傕側傫偱傕柍偄偱
偡偹丅嵟嬤偺 HDD 傗 MO 偺婰榐枾搙傪峫偊傞偲乯CD-ROM 偼丄壒妝儗僐乕僪偲
摨偠偔梿慁忬偺僩儔僢僋傪帩偭偰偄傞揰偑帴婥僨傿僗僋偲堎側傞揰偱偡丅岝憡
曄壔僪儔僀僽偼丄僩儔僢僋傗僙僋僞偵暘妱偝傟偰偄傞揰偱偼丄岝僨傿僗僋偲偺
堘偄偼偁傝傑偣傫偑丄傛傝桪傟偨惈幙偑偁傝傑偡丅偳偆偄偆偙偲偐偲偄偆偲丄
岝帴婥僨傿僗僋偑楑壙偵偼僨乕僞偺僆乕僶乕儔僀僩偑弌棃側偄偺偵懳偟丄岝憡
曄壔僨傿僗僋偱偼壜擻偱偁傞偙偲丅傑偨丄岝憡曄壔儊僨傿傾偑丄帴婥傗揹壸偵
懳偟慡偔塭嬁傪庴偗側偄偺偱丄嬌傔偰挿庻柦偱偁傞偙偲側偳偱偡丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

2.2. 棙揰

 丒 500 僪儖埲壓偱偁傞偙偲丅乮栿拲丗尰嵼偼丄4 攞懍偱 30000 墌掱搙丠乯
   
 丒 婛偵 SCSI 僐儞僩儘乕儔傪帩偭偰偄傟偽丄崱偁傞傕偺偲堦弿偵丄傕偟偔偼
    梊旛偺僨傿僗僋偲偟偰棙梡偱偒傞傛偆偵側傝傑偡丅
   
 丒 撉傒彂偒壜擻側岝僨傿僗僋
   
 丒 4 攞懍偱 CD-ROM 偑撉傔傞丅
   
 丒 Kodak 偺 PhotoCD 偑撉傔傞丅
   
 丒 儊僨傿傾偼 15 擭偺庻柦偑偁傞丅
   
 丒 SCSI-2 僀儞僞乕僼僃乕僗偱偁傞丅
   
 丒 CD-ROM 偑梿慁忬偵婰榐偡傞偺偲堎側傝丄僩儔僢僋乛僙僋僞宍幃偺僼僅乕儅
    僢僩偱偁傞丅
   
 丒 傾僋僙僗僞僀儉 165ms - 僥乕僾傛傝梱偐偵懍偄丅
   
 丒 650MB 偺戝梕検儊僨傿傾偱偁傞丅
   
 丒 僨傿僗僋 1 枃栺 50 僪儖乮栿拲丗崱偼擔杮嫶偱偼 2600 墌偑晛捠乯
   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

2.3. 棟夝偟偰梸偟偄帠

 丒 僪儔僀僽偲堦弿偵攧偭偰偄傞 SCSI 僐儞僩儘乕儔偑丄Linux 偱摦嶌偡傞偐
    斲偐偼晄柧偱偡丅傕偟丄偦偺 SCSI 僐儞僩儘乕儔偐暿偺僐儞僩儘乕儔偑摦
    嶌偡傞偙偲偑敾偭偨傜丄惀旕巹偵儊乕儖傪憲偭偰壓偝偄丅
   
 丒 岝僨傿僗僋偺僼僅乕儅僢僩偼丄懠偺僨傿僗僋僪儔僀僽偺僼僅乕儅僢僩偲屳
    姺惈偼偁傝傑偣傫丅偟偐偟丄PC 梡偺師悽戙僪儔僀僽偱偁傞偺偵廫暘側僠儍
    儞僗偑偁傝傑偡丅
   
 丒 儀儞僟乕偼丄UNIX 傪僒億乕僩偡傞傛偆偵偼巚偊傑偣傫丅巆擮側偑傜丄 DOS
    /Windows 傗 Macintosh 傪懳徾偵偟偰偄傞傛偆偱偡丅
   
 丒 LUN 僕儍儞僷 7 斣偼丄AT 屳姺婡偱偼丄OFF 偵愝掕偟偰偍偔昁梫偑偁傝傑
    偡丅乮栿拲丗尨暥偱偼丄偳偪傜偱傕偄偄傛偆偵側偭偰傑偡偑丄娫堘偊傞偲
    尨暥偺傛偆偵丄CD-ROM 偲 PD 傪摨帪偵巊偊側偔側傝傑偡丅偦偺戙傢傝偵丄
    僕儍儞僷傪 MAC 儌乕僪偵偟偰偍偔偲丄嵟弶偵擖傟偰偍偄偨儊僨傿傾僞僀僾
    偺僪儔僀僽偲偟偰擣幆偟傑偡丅乯
   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

3. 僀儞僗僩乕儖

LF1000 偼丄SCSI-2 屳姺偺僨僶僀僗偱偡丅僽儘僢僋僒僀僘偼丄512 僶僀僩偱丄
Linux 偺 SCSI 僪儔僀僶偲屳姺惈偑偁傝傑偡丅偙偺僪儔僀僽傪丄Adaptec 1542C
SCSI 僐儞僩儘乕儔傪巊偭偰 AMD 486-100MHz 儅僔儞偵僀儞僗僩乕儖偟偰傒傑偟
偨丅僀儞僗僩乕儖偲丄撉傒彂偒壜擻側岝僨傿僗僋偺儅僂儞僩偼丄埲壓偵弎傋傞
傛偆側庤弴偱峴側偄傑偟偨丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

3.1. 僀儞僗僩乕儖偺庤弴

 丒 僪儔僀僽傪庢傝晅偗丄懠偺僨僶僀僗偲傇偮偐傜側偄傛偆偵 SCSI ID 傪僙僢
    僩偡傞丅偦偺屻丄働乕僽儖傪宷偓捈偡丅
   
 丒 僐儞僺儏乕僞傪婲摦偟丄SCSI 僐儞僩儘乕儔偑僪儔僀僽傪擣幆偟偰偄傞偙偲
    傪妋擣偡傞丅
   
 丒 Linux 偺僇乕僱儖偑婲摦偟偰偄傞娫偵丄SCSI 僨僶僀僗偑怴偨偵擣幆偝傟傞
    偙偲偲巚偄傑偡丅巹偺応崌偼丄/dev/sda 偵僴乕僪僨傿僗僋偑偁傞偺偱丄/
    dev/sdb 偲偟偰擣幆偝傟傑偟偨丅
   
 丒 overwrite warning 偑弌傞偺偱丄傑偨 dosemu 偺愝掕傪偄偠傝偨偔柍偐偭
    偨偺偱 fdisk 僐儅儞僪偼巊偄傑偣傫偱偟偨丅
   
 丒 劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
    劆  mkfs -t ext2 /dev/sdb                                 劆
    劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
   
 丒 劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
    劆  mkdir /pd                                             劆
    劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
   
 丒 劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
    劆  mount -t ext2 -o ro,suid,dev,exec,auto,nouser,async /dev/sdb /pd劆
    劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
    偲偡傟偽丄撉傒崬傒愱梡儅僂儞僩
   
 丒 劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
    劆  mount -t ext2 -o defaults /dev/sdb /pd                劆
    劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
    偲偡傟偽丄撉傒彂偒壜擻偱儅僂儞僩偱偡丅
   
偙傟偱弨旛偼姰椆偱偡丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

3.2. 僸儞僩

SCSI 僇乕僱儖僪儔僀僶偑丄CD-ROM ISO 9660 僼僅乕儅僢僩偲 ext2 僼僅乕儅僢
僩側偳偺僨僶僀僗儌乕僪偺曄峏傪僒億乕僩偟偰偄傞偐偳偆偐偼丄晄柧偱偡丅偳
側偨偐丄敾傝傑偟偨傜儊乕儖傪壓偝偄丅

栿拲丗彮側偔偲傕丄aic7xxx, ncr53c[7,8]xx, ncr53c8xx 側偳偺僪儔僀僶偱偼
丄壜擻偱偟偨丅僇乕僱儖傪丄LUN 傪専嶕偵偄偔傛偆偵嶌傝捈偡偐丄 boot
prompt 偱 max_scsi_luns=1 傪愝掕偡傞昁梫偼偁傝傑偡丅

曗懌丗屻弎偟傑偡偑嵟怴僇乕僱儖偱偼丄max_scsi_luns 偺愝掕偼柍娭學偱偡丅

Linux 偺僽乕僩帪偵丄偪傖傫偲僪儔僀僽傪擣幆偟偰偄傑偡偐丠 dmesg 偺弌椡偺
敳悎傪偮偗偰偍偒傑偡丅MATSHITA 僪儔僀僽傪擣幆偟偰偄傞偐偳偆偐妋擣偟偰壓
偝偄丅偨傇傫摨偠傛偆側儊僢僙乕僕偑弌傞敜偱偡丅

 

   
    拲堄揰: "Adding Swap" 偺壓 3 峴偼丄Linux 偑 PD 傪巊偊傞傛偆偵僽乕僩
    偟偨偨傔偱偡丅傕偟丄CD-ROM 傪 PD-Drive 偵擖傟偨傑傑僽乕僩偟偨応崌丄
    偙偺 CD-ROM 傪 iso9660 僼僅乕儅僢僩偺儊僨傿傾偲偟偰 /cdrom 偵儅僂儞
    僩偟傑偡丅CD-ROM 傪巊偭偰 Linux 傪僀儞僗僩乕儖偡傞応崌偵偼丄PD 僪儔
    僀僽偵 CD-ROM 傪擖傟偨傑傑僽乕僩偟側偔偰偼偄偗傑偣傫丅偄偭偨傫
    Linux 偑僽乕僩偟偨屻偼丄"umount /cdrom" 偲偡傞偙偲偱丄儊僨傿傾傪岎
    姺偱偒傑偡丅傕偪傠傫丄儅僂儞僩偟捈偝側偗傟偽偄偗傑偣傫丅埲壓偵丄偙
    偺憖嶌傪彆偗傞 Shell Script 傪梡堄偟偰偁傝傑偡丅"mgrpd" 偺柤慜偱僼
    傽僀儖偵愗傝偲傝丄"sh mgrpd" 偲偟偰幚峴偟偰壓偝偄丅
   
    乮栿拲丗僇乕僱儖媦傃 PD 僪儔僀僽偺 LUN 偺愝掕傪惓偟偔峴側偊偽丄愭偵
    CD-ROM 傪擖傟偰偍偙偆偑丄PD 傪擖傟偰偍偙偆偑丄偄偮偱傕丄mount,
    umount 張棟偱儊僨傿傾岎姺偼壜擻偱偡丅乯
   
  #-----------dmesg僐儅儞僪偺弌椡-------------------------------------            
  Configuring Adaptec at IO:330, IRQ 11, DMA priority 5                           
  scsi0 : Adaptec 1542                                                            
  scsi : 1 host.                                                                  
    Vendor: QUANTUM   Model: PD1050iS          Rev: 3110                          
    Type:   Direct-Access                      ANSI SCSI revision: 02             
                                                                                  
  Detected scsi disk sda at scsi0, id 0, lun 0                                    
    Vendor: MATSHITA  Model: PD-1 LF-1000      Rev: A109                          
    Type:   Optical Device                     ANSI SCSI revision: 02             
  Detected scsi disk sdb at scsi0, id 1, lun 0                                    
  scsi : detected 2 SCSI disks total.                                             
  SCSI Hardware sector size is 512 bytes on device sda                            
  SCSI Hardware sector size is 512 bytes on device sdb                            
  Linux version 1.2.13 (root@bigkitty) (gcc version 2.7.0) #1 Wed Aug 23 03:54:14 
                                                                                  
  CDT 1995                                                                        
  Partition check:                                                                
    sda: sda1 sda2 sda3 sda4                                                      
    sdb: bad partition table                                                      
  VFS: Mounted root (ext2 filesystem) read-only.                                  
  Adding Swap: 34812k swap-space                                                  
  end_request: I/O error, dev 2100, sector 64                                     
  isofs_read_super: bread failed, dev 0x2100 iso_blknum 16                        
  Unable to identify CD-ROM format.                                               
  #-------------------偙偙傑偱dmesg僐儅儞僪偺弌椡-----------------                

Adaptec 1542C SCSI 僐儞僩儘乕儔偺僪儔僀僶偼丄Slackware 偺 scsinet1 僇乕
僱儖偺傕偺傪巊偄傑偟偨丅偙偺僐儞僩儘乕儔偺応崌偼丄柍帠摦偒傑偟偨偑丄堘
偆僐儞僩儘乕儔傪巊偆応崌偼丄Drew Eckhardt 巵偺彂偄偨 SCSI-HOWTO (擔杮岅
栿 <http://www.linux.or.jp/JF/JFdocs/SCSI-HOWTO.html>) 傪尒偰壓偝偄丅

LF1000 僪儔僀僽傪巊偆忋偱曋棙側 Shell Script 傪埲壓偵晅婰偟偰偍偒傑偡丅
帺桼偵巊偭偰傕傜偭偰寢峔偱偡偑丄Copyright 昞帵偼巆偟偰偍偄偰偔偩偝偄丅
乮栿拲丗屻弎偡傞棟桼偱丄AT 屳姺婡偱偼偁傑傝栶偵棫偨側偄偱偡丅MkLinux 傪
摦偐偡応崌偵偼堄枴偑偁傞偐傕乯

  ------------------------偙偙偐傜--------------------------------                
  #@/@/@ mgrpd    ABR Linux 1.2.13 486  mgr shell for phase change drive          
  #************************************************************************#      
  #                                                                        #      
  #  program : mgrpd                                                       #      
  #                                                                        #      
  #                                                                        #      
  #                                                                        #      
  #                                                                        #      
  #       Author : Skip Rye  Copyright 1996                                #      
  #                                                                        #      
  #       Revision : v1.0  02-01-96 Start                                  #      
  #                        03-13-96 Released                               #      
  #                                                                        #      
  #       Calls : None                                                     #      
  #                                                                        #      
  #       Files :                                                          #      
  #                                                                        #      
  #                                                                        #      
  ########################################################################*/      
  # Display menu and process choice:                                              
  sel=0                                                                           
  while [ $sel ]                                                                  
  do                                                                              
     echo "***************************************************************"       
     echo "*                         MGRPD                               *"       
     echo "* Version v1.0, Copyright 1996, Author Skip Rye              *"        
     echo "***************************************************************"       
     echo "**************  ext2 formated file system *********************"       
     echo "1)  Format pd disk - mkfs /dev/sdb"                                    
     echo "2)  Mount pd read/write"                                               
     echo "3)  Mount pd read only"                                                
     echo "************** dos formated file system ***********************"       
     echo "Note : must have been formatted using dos"                             
     echo "4)  Mount read/write"                                                  
     echo "5)  Mount read only"                                                   
     echo "40)  List disk space - df"                                             
     echo "50)  umount"                                                           
     echo "######################## CDROM ################################"       
     echo "Note : must have Use LUN Numbers jumper on drive"                      
     echo "100) Mount CDROM"                                                      
     echo "101) umount CDROM"                                                     
     echo "END Hit  to End"                                                       
     echo                                                                         
     echo "Select option: \c"                                                     
                                                                                  
     read sel                                                                     
     case $sel in                                                                 
                                                                                  
     1)                                                                           
        echo "This option assumes ext2 is the default mkfs format"                
        echo "This will DESTROY ALL data on disk. Enter y to continue."           
        read ans1                                                                 
        if [ $ans1 ]                                                              
        then                                                                      
           echo "Enter the fully qualified path name of the PD drive"             
           echo "ie. /dev/sdb"                                                    
           read pdpath                                                            
           if [ $pdpath ]                                                         
           then                                                                   
              if [ $ans1 = "y" -o $ans1 = "Y" ]                                   
              then                                                                
                  echo "This will DESTROY ALL data on disk $pdpath. Enter y to co 
  ntinue"                                                                         
                  read ans2                                                       
                  if [ $ans2 ]                                                    
                  then                                                            
                    if [ $ans2 = "y" -o $ans2 = "Y" ]                             
                    then                                                          
                       mkfs $pdpath                                               
                    fi                                                            
                 fi                                                               
              fi                                                                  
           fi                                                                     
        fi                                                                        
     ;;                                                                           
     2)                                                                           
        mount -t ext2 -o defaults /dev/sdb /pd                                    
     ;;                                                                           
     3)                                                                           
        mount -t ext2 -o ro,suid,dev,exec,auto,nouser,async /dev/sdb /pd          
     ;;                                                                           
     4)                                                                           
        mount -t msdos -o rw,suid,dev,exec,auto,nouser,async /dev/sdb /pd         
     ;;                                                                           
     5)                                                                           
        mount -t msdos -o ro,suid,dev,exec,auto,nouser,async /dev/sdb /pd         
     ;;                                                                           
     40)                                                                          
        df                                                                        
     ;;                                                                           
     50)                                                                          
        umount /dev/sdb                                                           
     ;;                                                                           
     100)                                                                         
        /etc/rc.d/rc.cdrom                                                        
     ;;                                                                           
     101)                                                                         
        umount /cdrom                                                             
     ;;                                                                           
     esac                                                                         
  done                                                                            
                                                                                  
  ------------------偙偙傑偱----------------------------------                    

傕偟丄偆傑偔偄偐側偐偭偨応崌偼丄埲壓偺揰傪僠僃僢僋偟偰傒偰壓偝偄丅

 丒 SCSI 僐儞僩儘乕儔偼壗傪巊偭偰偄傑偡偐丠僒億乕僩偝傟偰偄傞僇乕僪偱偡
    偐丠 Drew Eckhardt 巵偺 SCSI-HOWTO (擔杮岅栿 <http://
    www.linux.or.jp/JF/JFdocs/SCSI-HOWTO.html>) 傪尒偰壓偝偄丅
   
 丒 SCSI 僐儞僩儘乕儔偺僪儔僀僶傪僇乕僱儖偵慻傒崬傫偱偄傑偡偐丠
   
埲壓 3 揰偼丄岆夝傪彽偔偺偱丄AT 屳姺婡儐乕僓乕偼撉傒旘偽偟偰壓偝偄丅

 丒 CD-ROM 傪巊偆偵偼丄Linux 偺僽乕僩慜偵 LF1000 偺揹尮傪擖傟丄CD-ROM
    傪擖傟偰偍偔昁梫偑偁傝傑偡丅CD-ROM 傪擣幆偱偒偨屻偵偼丄CD 傪傾儞儅
    僂儞僩偟丄 CD-ROM 傪庢傝懼偊偨傝丄儅僂儞僩偟捈偟偨傝偱偒傞傛偆偵側
    傝傑偡丅 -- "mgrpd" Shell Script 偺巊偄曽傪嶲徠偺偙偲丅
   
 丒 岝僨傿僗僋傪埖偆偵偼丄CD-ROM 傪擖傟偢偵 Linux 傪僽乕僩偟偰偔偩偝偄
    丅
   
 丒 LF1000 偺僕儍儞僷愝掕偼丄LUN 傪巊偆傛偆偵側偭偰偄傑偡偐丠
   
AT 屳姺婡儐乕僓乕偼丄埲壓偺揰傕僠僃僢僋偟偰壓偝偄丅

 丒 LF1000 僪儔僀僽偺揹尮偼擖偭偰偄傑偡偐丠
   
 丒 Kernel Configuration 偱 Probe all LUNs on each SCSI device 傪 on 偵
    偟偰僇乕僱儖傪嵞峔抸偟偰偁傝傑偡偐丠傕偟偔偼丄僽乕僩僾儘儞僾僩偱丄
    max_scsi_luns=1 傪愝掕偟傑偟偨偐丠 (栿拲丗嵟嬤偺僇乕僱儖偱偼丄Probe
    all LUNs on each SCSI device 偑 off 偺傑傑偱傕丄PD 偺 LUN 偼僒億乕
    僩偝傟傞傛偆偵側傝傑偟偨丅Kernel 2.0.22 埲崀偩偭偨傛偆偵巚偄傑偡)
   
 丒 LF1000 偺 LUN 僕儍儞僷 7 斣傪 off 偺埵抲偵崌傢偣偰偁傝傑偡偐丠
   
PD偺儊僨傿傾偼丄栺 500000 夞偺撉傒彂偒偑偱偒傞偦偆偱偡丅乮栿拲丗巹偺抦
傞偲偙傠偱偼 100 枩夞僆乕僟乕偱偡丅乯偟偐偟 Linux 側偳偺 OS 傪 PD 忋偵
僀儞僗僩乕儖偡傞偙偲偼姪傔傑偣傫丅偙偺傛偆側 OS 偼丄僾儘僙僗傪僨傿僗僋
偵彂偒崬傫偩傝撉傒崬傫偩傝偡傞傕偺偱偡丅偙偆偄偆巊偄曽偱偼丄娙扨偵儊僨
傿傾偺庻柦偑偔傞偙偲偵側偭偰偟傑偄傑偡丅

偱偒傞偩偗丄撉傒崬傒愱梡偱儅僂儞僩偡傞傛偆偵偟傑偟傚偆丅

彂偒崬傒偼丄戝偒側屌傑傝偺扨埵偱峴側偄傑偟傚偆丅偙傟偵傛偭偰丄撉傒崬傒
帪偺僔乕僋傪憹傗偡尦偲側傞僼儔僌儊儞僥乕僔儑儞傪尭彮偝偣傞偙偲偑偱偒傑
偡丅

偟偐偟側偑傜丄僶僢僋傾僢僾傗丄夋憸丄偁傑傝巊偆帠偺柍偄嫄戝僾儘僌儔儉偺
曐懚梡偵偼丄慺惏傜偟偄儊僨傿傾偱偡丅僶僢僋傾僢僾偐傜偺儕僗僩傾偼丄僥乕
僾傛傝傕壗攞傕崅懍偱偡丅僶僢僋傾僢僾偼丄僥乕僾僪儔僀僽偱偼栶偵棫偨側偄
"cp -rp"僐儅儞僪偱傕峴側偊傑偡丅偑丄偙偺応崌偼丄僔儞儃儕僢僋儕儞僋偑幚
僼傽僀儖偵抲偒姺傢偭偰偟傑偄傑偡丅

劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

4. 捛壛丒曗懌

偙偺愡偼丄栿幰偺彑庤側捛壛帠崁偱偡丅

巹偺抦偭偰偄傞尷傝丄PD 僪儔僀僽偺弌壸帪僨僼僅儖僩愝掕偼丄儔僀僩僉儍僢僔
儏偑僆僼偵側偭偰偄傑偡丅Panasonic 斉偵晅懏偺僣乕儖傪 DOS 忋偱摦偐偣偽儔
僀僩僉儍僢僔儏傪僆儞偺忬懺偱僙乕僽偱偒傑偡丅偱偡偑丄彮側偔偲傕丄僩乕儗
丒僽儔儞僪偵晅懏偺僣乕儖偱偼丄揹尮傪愗傞偨傃偵丄儔僀僩僉儍僢僔儏偑僆僼
偺忬懺偵弶婜壔偝傟傞偙偲偑妋擣偱偒偰偄傑偡丅

MO 偺儔僀僩僉儍僢僔儏偑僆儞偵側偭偰偄傞忬懺偱丄Win95 側偳偺廮側 OS 忋偱
巊梡偡傞偲丄戝検偺僼傽僀儖傪僐僺乕偡傞応崌偵僔僗僥儉偑僴儞僌偟偨傝偡傞
偙偲傕偟偽偟偽偱偡偑丄PD 偺応崌偼丄偦偺傛偆側帠懺偑敪惗偟偨偙偲偼偁傝傑
偣傫偱偟偨丅乮帺暘帺恎傗桭恖払傪娷傔偰乯偳偆傕丄僪儔僀僽偺僉儍僢僔儏傾
儖僑儕僘儉偺栤戣偺偣偄偱偼側偄偐偲悇應偝傟傑偡丅

偟偐偟丄Linux 忋偱偼丄戝偒側僼傽僀儖偺僐僺乕帪偵僔僗僥儉偑僴儞僌偟偨偲
偄偆曬崘傕偁傝傑偟偨偑丄JF-ML偱偺幚尡曬崘偵傛傟偽丄SCSI 僇乕僪偺宆斣丒
儕價僕儑儞偵傛偭偰婲偒傞壜擻惈偑偁傞傛偆偱偡丅

嶨帍側偳偱丄PD 偼 MO 偵斾傋偰彂偒崬傒偑抶偄偲彂偐傟偰偄傑偡偑丄彮側偔偲
傕丄PD 傕儔僀僩僉儍僢僔儏傪僆儞偵偡傟偽丄230M-MO 傛傝偼崅懍側寢壥偑弌偰
偄傑偡丅乮暋悢偺娐嫬偱乯

儔僀僩僉儍僢僔儏傪僆儞偺忬懺偱巊梡偟偨曽偑夣揔偵巊偊傞偲偼巚偄傑偡偑愭
偵彂偄偨栤戣偑婲偒傞応崌傕偁傞偺偱丄at your own risk 偱丄岲偒側曽偵愝掕
偟偰壓偝偄丅

傕偪傠傫丄FAT, VFAT 偱儅僂儞僩偡傞傛傝丄ext2 偱 makefs 偟偰 Linux 愱梡
偱巊偆傎偆偑夣揔偱偡丅(巹偼 2 戜偺 PD 偺堦戜傪 ext2丄堦戜傪 vfat 偱儅僂
儞僩偡傞傛偆側愝掕傪僨僼僅儖僩偵偟偰偄傑偡丅)惓妋偵寁應偼偟偰偄傑偣傫偑
丄彮側偔偲傕 4-5 攞偼崅懍偵側偭偨傛偆偵巚偊傑偡丅

儔僀僩僉儍僢僔儏偑僆儞偵側偭偰偄傞偐偳偆偐偼丄僼儘儞僩僷僱儖偺 LED 偑彂
偒崬帪偵僆儗儞僕怓偵側偭偰偄傞偐偳偆偐偱嬫暿偱偒傞傛偆偱偡丅乮悢幮偺惢
昳傪挷傋偨寢壥乯僆儗儞僕偵側傞側傜儔僀僩僉儍僢僔儏偼僆儞丄側傜側偗傟偽
丄儔僀僩僉儍僢僔儏偼僆僼偱偡丅堦搙偛妋擣偺傎偳傪丅

側偍丄Panasonic 埲奜偱丄儔僀僩僉儍僢僔儏側偳偺弶婜愝掕忣曬傪丄婰壇偝偣
傜傟傞僣乕儖傪晅懏偟偰偄傞傕偺偼丄偁傞偺偐偳偆偐晄柧偱偡丅偝偡偑偵岎桭
娭學偩偗偱丄奺幮偺僪儔僀僽傪挷傋傞偵偼尷搙偑偁傝傑偡丅

乽偆偪偺偼晅偄偰偨乿乽偆偪偺偵偼晅偄偰側偐偭偨乿偲偄偭偨忣曬傪嫵偊偰偔
偩偝偄丅

1997/4/30 尰嵼丄WWW丄ftp 側偳偱丄Panasonic Tools 傪擖庤偡傞曽朄偼柍偄傛
偆偱偡丅Panasonic 偑岞奐偟偰偔傟傞偙偲傪婅偭偰偄傑偡丅

